REACH - Chemical Regulation

Page Content

 **REACH, Regulation No 1907/2006 on the Registration, Evaluation, Authorisation and Restriction of Chemicals.**
REACH requires that sufficient information on Substances of Very High Concern (SVHC) contained in articles in concentration above 0.1% weight by weight (w/w) is communicated to allow the safe use of the product.

The following tables cover 191 REACH SVHCs which are updated by ECHA on 27th June, 2018. (http://echa.europa.eu/candidate-list-table)

**The following products contain a SVHC in a concentration above 0.1% w/w.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  Product | Description | Substance Name | EC No. | Information on safe use |
| BP71GA3 | Glossy A3 Photo Paper | Boric acid | 233-139-2 | Do not allow to come into contact with mouth. |
| BP71GA4 | Glossy A4 Photo Paper | Boric acid | 233-139-2 | Do not allow to come into contact with mouth. |
| BP71GP20 BP71GP50 | Glossy 10cm x 15cm Photo Paper | Boric acid | 233-139-2 | Do not allow to come into contact with mouth. |
| BA-9000  | BATTERY FOR PT-9600 | Bis (2-ethylhexyl)phthalate (DEHP) | 204-211-0 | Do not keep the battery cover open. |
|  |  |  |  |  |
| Carton boxes  | AiRScouter 300 series | Tetraboron disodium heptaoxide, hydrate | 235-541-3 | Do not allow to come into contact with mouth. |
| Carton box for specific toner cartridges (\*1) | Outer Carton for toner cartridges | Disodium tetraborate decahydrate | 215-540-4 | Do not allow to come into contact with mouth. |
| Carton box for Supply Inkjet head unit (\*2) | Inner carton for protecting head unit | Disodium tetraborate decahydrate | 215-540-4 | Do not allow to come into contact with mouth. |

\*1:

TN-329C P, TN-329BK P, TN-329M P, TN-329Y P, TN-900C P, TN-900BK P, TN-900M P, TN-900Y P, TN-900C MPS, TN-900BK MPS, TN-900M MPS, TN-900Y MPS

\*2:

PRINT HEAD SUPPLY UNIT M17HT (D00STP001), PRINT HEAD SUPPLY UNIT S13(LK6584001)

**The items below may contain substances above the threshold at an individual component level but not above 0.1%(w/w) of the total article weight.**

| Item | Product | Substance Name | EC No. | Information on safe use |
| --- | --- | --- | --- | --- |
| Inkjet head actuator | All of the inkjet “All in One” printers | Lead titanium zirconium oxide | 235-727-4 | Do not break inkjet head units |
| Flexible Flat cable of thermal head | MW-145BT | 1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene ("Dechlorane Plus"TM) | 236-948-9 | Do not break to open device cover |
| HD cable | AiRScouter WD-350 | 1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene ("Dechlorane Plus"TM) | 236-948-9 | Do not break cable cover |
| Solenoid for print mechanism | See the model names in the following footnote (\*3) | 1,6,7,8,9,14,15,16,17,17,18,18-Dodecachloropentacyclo[12.2.1.16,9.02,13.05,10]octadeca-7,15-diene ("Dechlorane Plus"TM) | 236-948-9 | Do not break to open device cover |
| Copper alloy Plugs for Power Cord  | All Printers, All in One printers, Fax machines, P Touch products, QL Products, Stamp Creator and PocketJet | Lead | 231-100-4 | Keep out of the reach of children. |
| Copper alloy Motor Gear  | All Printers, All in One printers, Fax machines, P Touch products, QL Products, Stamp Creator and PocketJet | Lead | 231-100-4 | Keep out of the reach of children. |
| Copper alloy Motor Sleeve  | All Printers, All in One printers, Fax machines, P Touch products, QL Products, Stamp Creator and PocketJet | Lead | 231-100-4 | Keep out of the reach of children. |
| Parts containing iron shaft  | All Printers, All in One printers, Fax machines, P Touch products, QL Products, Stamp Creator and PocketJet | Lead | 231-100-4 | Keep out of the reach of children. |
| Liquid Crystal Display unit | See the model names in the following footnote (\*4) | Tetraboron disodium heptaoxide, hydrate | 235-541-3 | Do not break the Liquid Crystal Display Panel. |
| Liquid Crystal Display Cover | TP-M5000N“TapeCreator” | 2-(2H-benzotriazol-2-yl)-4,6-ditertpentylphenol (UV-328) | 247-384-8 | Do not break the Liquid Crystal Display Panel. |

\*3:

MFC-L3770CDW, DCP-1622WE, DCP-1623WE, DCP-1610W, DCP-1610WE, DCP-1612W, DCP-1612WE, DCP-1610WVB, DCP-1612WVB, MFC-1910W, MFC-1910WE, HL-1210W, HL-1210WE, HL-1212W, HL-1212WE, HL-1210WVB, HL-1212WVB, HL-1222WE, HL-1223WE, HL-1110, HL-1110E, HL-1112, HL-1112E, DCP-1510, DCP-1510E, DCP-1512, DCP-1512E, MFC-1810, MFC-1810E

\*4:

ADS-1600W, DCP-J552DW, DCP-J752DW, MFC-J650DW, MFC-J870DW, MFC-J6520DW, MFC-J6720DW, MFC-L2740DW, MFC-L2720DW, MFC-J491DW, MFC-J775DW, MFC-J480DW